UNAL\_MZS\_C6807\_XL#conf

UNAL\_MZS\_C6807\_XL#sh runn

Building configuration...

Current configuration : 14239 bytes

!

! Last configuration change at 13:13:01 UTC Tue Mar 19 2019

!

version 15.5

service timestamps debug datetime msec

service timestamps log datetime msec

no service password-encryption

service counters max age 5

!

hostname UNAL\_MZS\_C6807\_XL

!

boot-start-marker

boot system flash bootdisk:

boot-end-marker

!

!

enable secret 5 $1$WokM$dfX0uOyjycKPwZ3Ltv1zZ.

!

no aaa new-model

platform ip cef load-sharing ip-only

!

!

no ip domain-lookup

!

spanning-tree mode rapid-pvst

spanning-tree extend system-id

!

!

power redundancy-mode combined

!

redundancy

main-cpu

auto-sync running-config

mode sso

!

vlan internal allocation policy ascending

vlan access-log ratelimit 2000

!

!

class-map match-any class-copp-icmp-redirect-unreachable

class-map match-all class-copp-glean

class-map match-all class-copp-receive

class-map match-all class-copp-options

class-map match-all class-copp-broadcast

class-map match-all class-copp-mcast-acl-bridged

class-map match-all class-copp-slb

class-map match-all class-copp-mtu-fail

class-map match-all class-copp-ttl-fail

class-map match-all class-copp-arp-snooping

class-map match-any class-copp-mcast-copy

class-map match-any class-copp-ip-connected

class-map match-any class-copp-match-igmp

match access-group name acl-copp-match-igmp

class-map match-all class-copp-unknown-protocol

class-map match-any class-copp-vacl-log

class-map match-all class-copp-mcast-ipv6-control

class-map match-any class-copp-match-pimv6-data

match access-group name acl-copp-match-pimv6-data

class-map match-any class-copp-mcast-punt

class-map match-all class-copp-unsupp-rewrite

class-map match-all class-copp-ucast-egress-acl-bridged

class-map match-all class-copp-ip-admission

class-map match-any class-copp-dpss-divert

class-map match-all class-copp-service-insertion

class-map match-all class-copp-mac-pbf

class-map match-any class-copp-match-mld

match access-group name acl-copp-match-mld

class-map match-all class-copp-ucast-ingress-acl-bridged

class-map match-all class-copp-dhcp-snooping

class-map match-all class-copp-wccp

class-map match-all class-copp-nd

class-map match-any class-copp-ipv6-connected

class-map match-all class-copp-mcast-rpf-fail

class-map match-any class-copp-match-ndv6hl

match access-group name acl-copp-match-ndv6hl

class-map match-any class-copp-ucast-rpf-fail

class-map match-all class-copp-mcast-ip-control

class-map match-any class-copp-match-pim-data

match access-group name acl-copp-match-pim-data

class-map match-any class-copp-match-ndv6

match access-group name acl-copp-match-ndv6

class-map match-any class-copp-mcast-v4-data-on-routedPort

class-map match-any class-copp-mcast-v6-data-on-routedPort

!

policy-map policy-default-autocopp

class class-copp-mcast-v4-data-on-routedPort

police rate 10 pps burst 1 packets conform-action drop exceed-action drop

class class-copp-mcast-v6-data-on-routedPort

police rate 10 pps burst 1 packets conform-action drop exceed-action drop

class class-copp-dpss-divert

police rate 1000 pps burst 1000 packets conform-action transmit exceed-action drop

class class-copp-match-mld

police rate 5000 pps burst 5000 packets conform-action set-discard-class-transmit 48 exceed-action drop

class class-copp-match-igmp

police rate 5000 pps burst 5000 packets conform-action set-discard-class-transmit 48 exceed-action drop

class class-copp-icmp-redirect-unreachable

police rate 100 pps burst 10 packets conform-action transmit exceed-action drop

class class-copp-ucast-rpf-fail

police rate 100 pps burst 10 packets conform-action transmit exceed-action drop

class class-copp-vacl-log

police rate 2000 pps burst 1 packets conform-action transmit exceed-action drop

class class-copp-mcast-punt

police rate 1000 pps burst 256 packets conform-action transmit exceed-action drop

class class-copp-mcast-copy

police rate 1000 pps burst 256 packets conform-action transmit exceed-action drop

class class-copp-ip-connected

police rate 1000 pps burst 256 packets conform-action transmit exceed-action drop

class class-copp-ipv6-connected

police rate 1000 pps burst 256 packets conform-action transmit exceed-action drop

class class-copp-match-pim-data

police rate 1000 pps burst 1000 packets conform-action transmit exceed-action drop

class class-copp-match-pimv6-data

police rate 1000 pps burst 1000 packets conform-action transmit exceed-action drop

class class-copp-match-ndv6hl

police rate 10 pps burst 1 packets conform-action drop exceed-action drop

class class-copp-match-ndv6

police rate 1000 pps burst 1000 packets conform-action set-discard-class-transmit 48 exceed-action drop

!

!

!

!

!

interface GigabitEthernet1/1

no ip address

!

interface GigabitEthernet1/2

no ip address

shutdown

!

interface GigabitEthernet1/3

no ip address

shutdown

!

interface GigabitEthernet1/4

no ip address

shutdown

!

interface GigabitEthernet1/5

no ip address

shutdown

!

interface GigabitEthernet1/6

no ip address

shutdown

!

interface GigabitEthernet1/7

no ip address

shutdown

!

interface GigabitEthernet1/8

no ip address

shutdown

!

interface GigabitEthernet1/9

no ip address

shutdown

!

interface GigabitEthernet1/10

no ip address

shutdown

!

interface GigabitEthernet1/11

no ip address

shutdown

!

interface GigabitEthernet1/12

no ip address

shutdown

!

interface GigabitEthernet1/13

switchport

switchport mode trunk

!

interface GigabitEthernet1/14

no ip address

shutdown

!

interface GigabitEthernet1/15

no ip address

shutdown

!

interface GigabitEthernet1/16

no ip address

shutdown

!

interface GigabitEthernet1/17

no ip address

shutdown

!

interface GigabitEthernet1/18

no ip address

shutdown

!

interface GigabitEthernet1/19

no ip address

shutdown

!

interface GigabitEthernet1/20

no ip address

shutdown

!

interface GigabitEthernet1/21

no ip address

shutdown

!

interface GigabitEthernet1/22

no ip address

shutdown

!

interface GigabitEthernet1/23

no ip address

shutdown

!

interface GigabitEthernet1/24

no ip address

shutdown

!

interface GigabitEthernet3/1

no ip address

shutdown

!

interface GigabitEthernet3/2

no ip address

shutdown

!

interface GigabitEthernet3/3

no ip address

shutdown

!

interface TenGigabitEthernet3/4

no ip address

shutdown

!

interface TenGigabitEthernet3/5

no ip address

shutdown

!

interface GigabitEthernet5/1

switchport

switchport mode trunk

!

interface GigabitEthernet5/2

no ip address

shutdown

!

interface GigabitEthernet5/3

no ip address

shutdown

!

interface GigabitEthernet5/4

no ip address

shutdown

!

interface GigabitEthernet5/5

no ip address

shutdown

!

interface GigabitEthernet5/6

no ip address

shutdown

!

interface GigabitEthernet5/7

no ip address

shutdown

!

interface GigabitEthernet5/8

no ip address

shutdown

!

interface GigabitEthernet5/9

no ip address

shutdown

!

interface GigabitEthernet5/10

no ip address

shutdown

!

interface GigabitEthernet5/11

no ip address

!

interface GigabitEthernet5/12

no ip address

shutdown

!

interface GigabitEthernet5/13

no ip address

shutdown

!

interface GigabitEthernet5/14

no ip address

shutdown

!

interface GigabitEthernet5/15

no ip address

shutdown

!

interface GigabitEthernet5/16

no ip address

shutdown

!

interface GigabitEthernet5/17

no ip address

shutdown

!

interface GigabitEthernet5/18

no ip address

shutdown

!

interface GigabitEthernet5/19

no ip address

shutdown

!

interface GigabitEthernet5/20

no ip address

shutdown

!

interface GigabitEthernet5/21

no ip address

shutdown

!

interface GigabitEthernet5/22

no ip address

shutdown

!

interface GigabitEthernet5/23

no ip address

shutdown

!

interface GigabitEthernet5/24

no ip address

shutdown

!

interface GigabitEthernet5/25

no ip address

shutdown

!

interface GigabitEthernet5/26

no ip address

shutdown

!

interface GigabitEthernet5/27

no ip address

shutdown

!

interface GigabitEthernet5/28

no ip address

shutdown

!

interface GigabitEthernet5/29

no ip address

shutdown

!

interface GigabitEthernet5/30

no ip address

shutdown

!

interface GigabitEthernet5/31

no ip address

shutdown

!

interface GigabitEthernet5/32

no ip address

shutdown

!

interface GigabitEthernet5/33

no ip address

shutdown

!

interface GigabitEthernet5/34

no ip address

shutdown

!

interface GigabitEthernet5/35

no ip address

shutdown

!

interface GigabitEthernet5/36

no ip address

shutdown

!

interface GigabitEthernet5/37

no ip address

shutdown

!

interface GigabitEthernet5/38

no ip address

shutdown

!

interface GigabitEthernet5/39

no ip address

shutdown

!

interface GigabitEthernet5/40

no ip address

shutdown

!

interface GigabitEthernet5/41

no ip address

shutdown

!

interface GigabitEthernet5/42

no ip address

shutdown

!

interface GigabitEthernet5/43

no ip address

shutdown

!

interface GigabitEthernet5/44

no ip address

shutdown

!

interface GigabitEthernet5/45

no ip address

shutdown

!

interface GigabitEthernet5/46

no ip address

shutdown

!

interface GigabitEthernet5/47

no ip address

shutdown

!

interface GigabitEthernet5/48

no ip address

shutdown

!

interface Vlan1

description default

ip address 10.168.1.1 255.255.255.0 secondary

ip address 10.15.20.200 255.255.255.0

ip helper-address 168.176.195.217

no ip redirects

shutdown

!

interface Vlan33

no ip address

shutdown

!

interface Vlan42

no ip address

shutdown

!

interface Vlan47

no ip address

ip helper-address 192.168.80.2

shutdown

!

interface Vlan49

no ip address

shutdown

!

interface Vlan50

ip address 10.176.195.1 255.255.255.0

no ip redirects

shutdown

!

interface Vlan60

description RESIDENCIAS-G

no ip address

ip helper-address 192.168.80.2

shutdown

!

interface Vlan64

description salones-estu

no ip address

shutdown

!

interface Vlan65

no ip address

shutdown

!

interface Vlan71

description UNISALUD

ip address 192.168.71.254 255.255.255.0

shutdown

!

interface Vlan80

description server

no ip address

shutdown

!

interface Vlan83

description Laboratorio CISCO

no ip address

ip helper-address 192.198.80.2

shutdown

!

interface Vlan85

no ip address

shutdown

!

interface Vlan90

no ip address

shutdown

!

interface Vlan91

no ip address

shutdown

!

interface Vlan97

description Aulamultimedia

no ip address

ip helper-address 192.168.80.2

shutdown

!

interface Vlan100

description subred-Mgmtwlc

ip address 10.20.20.1 255.255.255.0

shutdown

!

interface Vlan101

description Subred-WLAN\_MAC

ip address 192.168.50.1 255.255.255.0

ip helper-address 192.168.80.2

shutdown

!

interface Vlan102

description Subred-WLAN\_LDAP

no ip address

shutdown

!

interface Vlan103

ip address 168.176.199.241 255.255.255.248

shutdown

!

interface Vlan105

description WLAN-Consacad

ip address 192.168.60.1 255.255.255.0

ip helper-address 192.168.80.2

shutdown

!

interface Vlan106

no ip address

ip helper-address 192.168.80.2

shutdown

!

interface Vlan107

no ip address

shutdown

!

interface Vlan110

no ip address

shutdown

!

interface Vlan111

no ip address

shutdown

!

interface Vlan150

description SIP

no ip address

shutdown

!

interface Vlan200

ip address 168.176.175.50 255.255.255.248

shutdown

ipv6 address 2800:8A0:8000:200::50/64

ipv6 enable

!

interface Vlan328

ip address 10.207.193.200 255.255.255.0

!

interface Vlan333

no ip address

shutdown

!

interface Vlan393

description DMZ

no ip address

ip helper-address 192.168.80.2

shutdown

!

interface Vlan394

description DMZ

no ip address

ip helper-address 192.168.80.2

shutdown

!

interface Vlan440

description LAPs-Auditorios

no ip address

shutdown

!

interface Vlan450

no ip address

no ip redirects

shutdown

!

interface Vlan451

ip address 192.168.40.1 255.255.254.0

ip helper-address 192.168.80.2

no ip redirects

ip pim sparse-dense-mode

shutdown

!

interface Vlan452

ip address 192.168.28.1 255.255.252.0

ip helper-address 192.168.80.2

no ip redirects

ip pim sparse-dense-mode

shutdown

!

interface Vlan453

description Subred-LAPs

no ip address

shutdown

!

interface Vlan454

no ip address

ip helper-address 192.168.80.2

shutdown

!

interface Vlan455

no ip address

shutdown

!

interface Vlan456

no ip address

ip helper-address 192.168.80.2

no ip redirects

shutdown

!

interface Vlan457

description Videobeams

ip address 192.168.56.1 255.255.255.0

ip helper-address 192.168.80.2

shutdown

!

interface Vlan458

description Camaras

no ip address

shutdown

!

interface Vlan459

no ip address

shutdown

ipv6 address 2800:8A0:8000:459::1/64

ipv6 enable

!

interface Vlan469

description Canopy

ip address 169.254.1.1 255.255.255.0

shutdown

!

interface Vlan501

description Camaras

no ip address

shutdown

!

interface Vlan555

no ip address

shutdown

!

interface Vlan601

no ip address

shutdown

!

ip default-gateway 10.207.193.117

ip forward-protocol nd

!

no ip http server

no ip http secure-server

!

ip access-list extended acl-copp-match-igmp

permit igmp any any

ip access-list extended acl-copp-match-pim-data

deny pim any host 224.0.0.13

permit pim any any

!

!

snmp-server community chicken RO

snmp-server community little RW

snmp-server location Data Center

snmp-server contact Soporte Redes

!

!

ipv6 access-list acl-copp-match-mld

permit icmp any any mld-report

permit icmp any any mld-query

permit icmp any any mld-reduction

permit icmp any any 143

!

ipv6 access-list acl-copp-match-ndv6

permit icmp any any nd-na

permit icmp any any nd-ns

permit icmp any any router-advertisement

permit icmp any any router-solicitation

permit icmp any any redirect

!

ipv6 access-list acl-copp-match-ndv6hl

permit icmp any any nd-na hoplimit

permit icmp any any nd-ns hoplimit

permit icmp any any router-advertisement hoplimit

permit icmp any any router-solicitation hoplimit

permit icmp any any redirect hoplimit

!

ipv6 access-list acl-copp-match-pimv6-data

deny 103 any host FF02::D

permit 103 any any

!

control-plane

service-policy input policy-default-autocopp

!

!

!

line con 0

password c3c0m

login

line aux 0

line vty 0 4

session-timeout 120

password c3c0m

login

transport input none

!

diagnostic bootup level minimal

no event manager policy Mandatory.go\_switchbus.tcl type system

!

end

UNAL\_MZS\_C6807\_XL#

UNAL\_MZS\_C6807\_XL#

UNAL\_MZS\_C6807\_XL#

UNAL\_MZS\_C6807\_XL#

UNAL\_MZS\_C6807\_XL#

UNAL\_MZS\_C6807\_XL#